HOMEWORK NETWORK

PART1

Step 3: .

**After you exit user EXEC mode, the switch will prompt you for a password to access the console interface and will prompt you a second time when accessing the privileged EXEC mode. You can also use the show run command to view the passwords.**

### Step 4:

**S1(config)# exit (or end)**

**S1# copy run start**

**PART 2:**

**Step2:**

**Your ping should have been unsuccessful because the switches have not been configured with an ip address.**

## **Part 3:**

### Step 1: Configure S1 with an IP address.

### Copy unning-config startup-config.to connect remotely to a switch,you need to assing an ip address to it.the default configuration on the switch is to have the management of the switch controlled through vlan1.

### Step 4: Save configurations for S1 and S2 to NVRAM.